0x0006 Route Group ID

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message
0x1E Generic PPL ICB in Route Control message

Byte | Description
0, 1 | Tag 0x0006
2, 3 | Length 0x0002
4, 5 | Value[0-1] Route Group ID or 0x0000 Null

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
See Information Control Block.