TCAP TUSI Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | PPL Event Indication format | 0x00=Use RAW CGPA and CDPA format in PPL Event Indication. (default) 0x01=Use CGPA and CDPA Elements format in PPL Event Indication
0x02 | User Abort Reason to use when a TCAP Transaction Abort is initiated (due to an Matrix Controller rest or switchover) | 0x00 (default)
0x03 | Action taken by TCAP when a subsystem is out-of-service | 0x00=Do not initiate TCAP restart when subsystem out-of-service 0x01=Initiate TCAP restart when subsystem out-of-service (default)
0x04-0x05 | Maximum length of the TC-primitive ICBs in PPL Event Indications | 0xFF (default)
0x06 | Action for dialog when timeout occurs | 0x00 Do not abort the dialog 0x01 Abort the dialog
0x07 | Abort reason when dialog timeout occurs | User defined
0x08 | Action to be taken when an SS7 card switchover occurs | 0x00 TCAP restart is not initiated (Keep all TCAP dialogs) 0x01 Initiate TCAP restart after SS7 switchover to reset TCAP dialogs
0x09 | Unused |
0x0A | Mandatory parameter validation | 0x00 - Disable 0x01 - Enable (Default)
0x0B | Configures whether the Dialogue Terminated Parameter TLV will be included in the last TCAP indication of a dialog. | 0x00 - Exclude TLV (Default) 0x01 - Include TLV
0x0C-0x11 | Reserved (Do Not Use) |
0x12 | ICB format for indications | 0x00 - Data ICB (default) 0x01 - Extended ICB format
0x13-0xC8 | Reserved (Do Not Use) |

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Transaction Capability Application Part.
See Signaling System Number Seven.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Information Control Block.