ISDN

Comp ID | Comp. Name | PPL Assign | PPL Audit Config. | PPL Audit Query | PPL Config. | PPL Data Query | PPL Event Request | PPL Timer Config.
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x0005 | L3P CC | Channel, D (0x0D) † | Channel, B (0x0D) | Channel, D (0x0D) | Channel, B (0x0D) | Channel, D (0x0D)
0x0006 | L3P DSM | Channel, D only (0x0D) | N/A | Channel, D only (0x0D)
0x0007 | L3P BSM | Channel, B only (0x0D) | Channel, B only (0x0D)
0x0008 | L3 CR | Channel, D (0x0D) † | Channel, B (0x0D) |  | Channel, D (0x0D) | Channel, B (0x0D) | Channel, D (0x0D)
0x0009 | L3 GCR | Channel, D only (0x0D) | N/A | Channel, D only (0x0D)
0x000A | L3 DSM | Channel, D only (0x0D) | Channel, D only (0x0D)
0x000B | L3 BSM | Channel, D (0x0D) † | Channel, B (0x0D) | Channel, D (0x0D) | Channel, B (0x0D) | Channel, D (0x0D))
† In these cases, the PPL components are instantiated on a per call basis and the PPL assignment is made to the controlling D channel. All subsequent calls then use the newly assigned L3P CR and/or L3 CR component.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.