# 4 Common Channel Signaling Cards

Purpose

This chapter provides descriptions of the Common Channel Signaling (CCS) cards.

Compliance

The Common Channel Signaling cards comply with all relevant regulations from the following standards organizations and governing bodies.

Country/Standards Organization | Regulations
--- | ---
United States and Canada | FCC Part 15 and ICES 003 CSA C22.2 No. 60950-1-3 CB Scheme IEC 60950-1
NEBS | NEBS Level 3 (GR-1089-CORE, GR-63-CORE)
European Union (CE Mark) | EN 55022: 1998/A1:2000/A2:2003 EN 55024: 1998/A1:2000/A2:2003 EN 300 386: Version 1.3.3 EN 60950-1
Australia/New Zealand | AS/NZS CISPR 22:2002 AS/NZS 60950.1:2003

In this section:

Dialogic® Common Channel Signaling I/O Card - EXS-CCS-1000/EXS-CCS-1000R

Dialogic® CCS I/O Series 3 Card - EXS7IO1300/EXS7IO1300R

CCS I/O Redundancy Cable Assembly - Part Nos. 64012301/ 164012301

CCS I/O Series 3 Red Cable - Part Nos. 64333300/164333300

Dialogic® ISDN PRI Card - LNX-PRI-1100

Dialogic® ISDN PRI Redundant I/O Card - LNXPIO1000

Dialogic® ISDN Series 3 Card - EXS-PRI-1300/EXS-PRI-1300R

Dialogic® Signaling System #7 PQ Card - See Model Numbers

Dialogic® Signaling System #7 Series 3 Card - See Model Numbers

CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
See Common Channel Signaling.
See Converged Services Administrator.
See Application Server.