Comp. ID | CompName | PPL Assign | PPL Audit Config | PPL Audit Query | PPL Config | PPL Data Query | PPL Event Req | PPL Event Ind | PPL Timer Config
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
0x000F | L3P CIC | Channel (0x0D) | CIC (0x3C)/ Channel (0x0D) | Channel (0x0D)
0x0010 | L3P Link | Link | N/A | Link (0x09)
0x0012 | ISUP CPC | Channel (0x0D)
0x0013 | ISUP SPRC | Stack (0x08) | N/A | Stack (0x08) | Stack (0x08)/Channel (0x0D) | Stack (0x08)
Channel (0x0D)
0x0014 | ISUP CCI | Channel (0x0D) | N/A | Channel (0x0D)
0x0015 | ISUP CRI
0x0016 | ISUP BLS
0x0017 | ISUP BLR
0x0018 | ISUP CRS
0x0019 | ISUP CRR
0x001A | ISUP UCIC
0x0042 | ISUP HLB
0x0043 | ISUP HRB
0x0044 | ISUP CRCR
0x001B | ISUP CGRS | N/A | N/A | Channel (0x0D) | N/A | Channel (0x0D)
0x001C | ISUP CGRR
0x001D | ISUP GBUS
0x001E | ISUP GBUR
0x001F | ISUP HGBR
0x0045 | ISUP MGBS
0x0046 | ISUP MGBR
0x0047 | ISUP HGBS
0x0076 | ISUP CQS
0x0077 | ISUP CQR
0x0078 | ISUP CVS | Channel (0x0D) | Channel (0x0D)
0x0079 | ISUP CVR
0x0081 | ISUP CRCS
0x0082 | ISUP DCO
0x0083 | ISUP CRO
0x0085 | ISUP SSC
0x00A8 | ISUP ACC | N/A | N/A | N/A | SS7 Destination (0x1C) | N/A | SS7 Destination (0x1C)
0x0011 | L3P TUP | Channel (0x0D) | Channel (0x0D)
0x0052 | TUP CPC
0x0053 | TUP SPRC | Stack (0x08) | Stack (0x08)
0x0054 | TUP BLR | Channel (0x0D) | Channel (0x0D)
0x0055 | TUP BLS
0x0057 | TUP CRI
0x0058 | TUP CRS
0x0059 | TUP CGRR | N/A | Channel (0x0D) | N/A | N/A | Channel (0x0D)
0x005A | TUP CGRS
0x005B | TUP MBUS
0x005C | TUP MBUR
0x005D | TUP HBUS
0x005E | TUP HBUR
0x005F | TUP SBUS
0x0060 | TUP SBUR
0x0020 | MTP2 AERM | Link (0x09) | N/A | Link (0x09)
0x0021 | MTP2 CC
0x0022 | MTP2 IAC
0x0023 | MTP2 LSC
0x0024 | MTP2 RC
0x0025 | MTP2 SURM
0x0026 | MTP2 TXC
0x002B | MTP3 HMDT * | Stack (0x08) | Stack (0x08)
0x002C | MTP3 HMRT **
0x002D | MTP3 LLSC
Notes: * When events 0x0005 Receive MSU Discarded and 0x0006 UPU MSU Received are received, the AIB is Destination (0x1C). ** When events 0x0003 Q.752 Destination Report, 0x0005 Transmit MSU Discarded and, 0x0006 UPU MSU Transmitted are received, the AIB is Destination (0x1C).
0x002E | MTP3 LSAC | Link (0x09) | N/A | Link (0x09)
0x0032 | MTP3 RCAT | Destination (0x1C) | Destination (0x1C)
0x0033 | MTP3 RSRT | Route (0x1D) | Route (0x1D)
0x0034 | MTP3 RTAC
0x0035 | MTP3 RTCC | Stack (0x08) | Stack (0x08)
0x0036 | MTP3 RTPC | Route (0x1D) | Route (0x1D)
0x0037 | MTP3 RTRC | Stack (0x08) | Stack (0x08)
0x0038 | MTP3 TCBC | Link (0x09) | Link (0x09)
0x0039 | MTP3 TCOC
0x003A | MTP3 TCRC | Route (0x1D) | Route (0x1D)
0x003C | MTP3 TLAC | Link (0x09) | Link (0x09)
0x003D | MTP3 TPRC | Stack (0x08) | Stack (0x08)
0x003E | MTP3 TRCC | Destination (0x1C) | Destination (0x1C)
0x003F | MTP3 TSFC * | Stack (0x08) | Stack (0x08)
0x0040 | MTP3 TSRC
* When events 0x0001 Destination Inaccessible and 0x0002 Destination Accessible are received, the AIB is Destination (0x1C).
0x0041 | MTP3 SLTC | Link (0x09) | N/A | Link (0x09)
0x0065 | SCCP SCLC | Stack (0x08) | Stack (0x08) | N/A | Stack (0x08)
0x0066 | SCCP SCRC
0x0067 | SCCP SUSI | Subsystem Number (0x2A)
0x0068 | SCCP SPPC | N/A
0x0069 | SCCP SPAC
0x006A | SCCP SPCC
0x006B | SCCP SSPC
0x006C | SCCP SSAC
0x006D | SCCP SSTC
0x006E | SCCP BCST
0x006F | SCCP LBCS
0x0070 | TCAP TUSI | Subsystem Number (0x2A)
0x0071 | TCAP CCO | N/A
0x0072 | TCAP ISM | N/A
0x0073 | TCAP TCO | Stack (0x08)
0x0074 | TCAP TSM | N/A
0x0075 | TCAP DHA |

SS7

See Programmable Protocol Language.
See Circuit Identification Codes.
See Integrated Services Digital Network User Part.
See Signaling System Number Seven.
Telephone User Part
Message Transfer Part level 2 - data link level
Message Transfer Part level 3 - network level
See Address Information Block.
See Transaction Capability Application Part.