0x05E5 Barge In

Use this TLV in the Play File Start and Resource Create message to enable barge-in for recorded files or a conference broadcast.

Byte | Description
0, 1 | Tag: 0x05E5 Barge In
2, 3 | Length: 0x0001
4 | Value[0]: Barge In Flag Bit 0 0 = Barge In Disabled (default for Play files) 1 = Barge In Enabled (default for conferencing (broadcast) Bit 1-7 Reserved (should be set to 0x00)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Message delimiter (SS7 bit pattern - 01111110)