L3P CIC PPL Event Requests (ITU)

The following table shows the PPL Event Requests supported by ITU ISUP L3P CIC.

Event ID | Event
--- | ---
0x01 | Send ACM
0x02 | Send CPG
0x03 | Send ANM
0x04 | Request local maintenance blocking (sends BLO)
0x05 | Request local maintenance group blocking (sends CGB)
0x06 | Request local maintenance unblocking (sends UBL)
0x07 | Request local maintenance group unblocking (sends CGU)
0x08 | Send GRS
0x09 | Send RSC
0x0A | Send HW block
0x0B | Send HW unblock
0x0C | Indicate CPC to wait for incoming COT report when the continuity check is being performed on the previous circuit
0x0D | Send incoming continuity check report when the continuity check was performed on the previous circuit.
0x0E | Send unrecognized message to the network. It is used for message pass on during MCP handling. NOTE: ICB subtype 0x1F should be used for sending the unrecognized message. DPC/CIC in the ICB should be sent as "00".
0x1E | Send CON
0x1F | Send CQM
0x20 | Send FAR
0x21 | Send FAA
0x22 | Send FRJ
0x23 | Send USR
0x24 | Send FAC
0x25 | Send PAM
0x26 | Send NRM
0x27 | Send CRG
0x28 | Send IDR
0x29 | Send IRS
0x2A | Send INR
0x2B | Send INF
0x2D | Send SUS
0x2E | Send RES
0x32 | Send SAM
0x33 | Reset timer T35 (for inbound SAM)
0x40 | Manual Stop (for Continuity re-checking)
0x41 | Send Continuity Check Request Message (CCR)
0x42 | Send UPT
0x43 | Send CCL
0x44 | Send OPR
0x46 | Send FOT
0x47 | Send DRS
0x49 | CMC Request with/without Parameters
0x4A | CMRJ request with/without Parameters.
0x4B | CMR Request with/without Parameters
0x4C | Request for COT
0x4D | Request for CCR
0x4E | Request for LPA
0x55 | Loop Prevention
0x60 | Send SGM

See Programmable Protocol Language.
International Telecommunications Union (UN)
See Integrated Services Digital Network User Part.
See Circuit Identification Codes.
See Information Control Block.
Destination Point Code
Continuity Check Request message (ISUP)