0x01DE ARP Cache Table Entry

This TLV is used in the ARP Cache Report message to report the IP Address and Ethernet Address for an entry in the ARP Cache table. Separate TLVs are sent or each entry in the table.

Byte | Description
0, 1 | Tag 0x01DE ARP Cache Table Entry
2, 3 | Length 0x000E
4-7 | Value[0-3] Entry Number
8-11 | Value[4-7] IP Address
12-17 | Value[8-13] Ethernet Address

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).