0x0605 EXS Conferencing Encoding Type

Use this TLV in the Resource Create (0x0124) message to specify the encoding type for a conference over the EXNET® ring.

Byte | Description
0, 1 | Tag: 0x0605 - EXS Conferencing Encoding Type
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Encoding Type 0x0000 - u-law 0x0001 - A-law 0x0002 - Mixed

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.