0x0695 FSK Modem Type

Use this TLV in the Outseize Control message.

Byte | Description
0, 1 | Tag: 0x0695 FSK Modem Type
2, 3 | Length (variable): 0x0002
4, 5 | Value[0,1]: Data Transmission Type 0x0000 - ITU V.23 (default) 0x0001 - Bell 202 0x0002 - Bell 202 Chinese

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Outgoing call setup during real-time call processing on a specific channel.
Frequency Shift Keying
International Telecommunications Union (UN)