MTP3 PPL Timers (ANSI)

This section contains default settings for ANSI PPL Timers, shown below by PPL component.

The MTP3 timers are accurate to 100 ms.

.

PPL Component | Timer ID | Spec/Timer | Default Value (10 ms)
--- | --- | --- | ---
RCAT (0x0032) | 0x01 | T1.111/T16 | 175
RSRT (0x0033) | 0x01 | T1.111/T10 | 4500
TCBC (0x0038) | 0x01 | T1.111/T3 | 80
0x02 | T1.111/T4 | 80
0x03 | T1.111/T5 | 80
TCOC (0x0039) | 0x01 | T1.111/T1 | 80
0x02 | T1.111/T2 | 140
TCRC (0x003A) | 0x01 | T1.111/T6 | 80
TPRC (0x003D) | 0x01 | T1.111/T22 | 6000
0x02 | T1.111/T23 | 1000
0x03 | T1.111/T26 | 1200
TRCC (0x003E) | 0x01 | T1.111/T15 | 250
TSRC (0x0040) | 0x01 | T1.111/T25 | 3000
0x02 | T1.111/T28 | 1000
0x03 | T1.111/T29 | 6000
SLTC (0x0041) | 0x01 | T1.111/T1 | 800

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
See Programmable Protocol Language.
Message Transfer Part level 3 - network level
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
ANSI Publication on Functional Description of MTP
Digital communications link - 44.378 Mbps rate