L3 D Channel Control Configuration Bytes

Byte | Description | Values
--- | --- | ---
0x01 | Channel ID encoding of extension bit | * 0x00 = Ext. bit set 0x01 = Ext. bit cleared
0x02 | Network Side (T309 Logic) Enable/Disable | 0x00 = Disable 0x01 = Enable Default is enabled if Connection Type is a Network Side variant.
0x09 | Send D channel Up event to GCR | 0x00 = Disable *0x01 = Enable

In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.