0x05F8 NFS Statistics

This TLV is included in the response to the Statistics Query message. It reports a wide range of NFS statistics for a specific DSP chip.

Byte | Description
0, 1 | Tag: 0x05F8 - NFS Statistics
2, 3 | Length: 0x005C
4 | Value[0] Module Number 0x00 - DSP Module 0 0x01 - DSP Module 1 0xFF - Main board
5 | Value[1]: Processor Number Valid Range - 0x00 - 0x03 0x00 for main board processor
6-9 | Value[2-5] :Total Reads
10-13 | Value[6-9]: Total Size of Reads
14-17 | Value[10-13]: Minimum Read Time Delay
18-21 | Value[14-17]: Maximum Read Time Delay
22-25 | Value[18-21]: Average Read Time Delay
26-29 | Value[22-25]: Total Writes
30-33 | Value[26-29]: Total Size of Writes
34-37 | Value[30-33]: Minimum Write Time Delay
38-41 | Value[34-37]: Maximum Write Time Delay
42-45 | Value[38-41]: Average Write Time Delay
46-49 | Value[42-45]: Total Opens
50-53 | Value[46-49]: Total Size of Opens
54-57 | Value[50-53]: Minimum Open Time Delay
58-61 | Value[54-57]: Maximum Open Time Delay
62-65 | Value[58-61]: Average Open Time Delay
66, 67 | Value[62, 63]: Simultaneous Files Being Played from Cache
68, 69 | Value[64, 65]: Max Simultaneous Files Being Played from Cache
70, 71 | Value[66, 67]: Average Simultaneous Files Being Played from Cache
72, 73 | Value[68, 69]: Simultaneous Files Playing & Filling the 8260 Cache
74, 75 | Value[70, 71]: Maximum Simultaneous Files Playing & Filling 8260 Cache
76, 77 | Value[72, 73]: Average Simultaneous Files Playing & Filling 8260 Cache
78, 79 | Value[74, 75]: Simultaneous Files Being Played Directly from NFS
80, 81 | Value[76, 77]: Maximum Simultaneous Files Being Played Directly from NFS
82, 83 | Value[78, 79]: Average Simultaneous Files Being Played Directly from NFS
84, 85 | Value[80, 81]: Simultaneous Files Being Written to 8260 Cache
86, 87 | Value[82, 83]: Maximum Simultaneous Files Being Written to 8260 Cache
88, 89 | Value[84, 85]: Average Simultaneous Files Being Written to 8260 Cache
90, 91 | Value[86, 87]: Simultaneous Files Being Written to the NFS Server
92, 93 | Value[88, 89]: Maximum Simultaneous Files Being Written to the NFS Server
94, 95 | Value[90, 91]: Average Simultaneous Files Being Written to the NFS Server

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor