MTP3 HMRT Configuration Bytes (ITU/ANSI)

Byte | Description | Value
--- | --- | ---
0x01 | Variant | 0x00=ANSI 0x01=ITU 0x02=Japan TTC/DDI 0x03=China 0x04=Japan NTT
0x02 | MSU Priority Filtering | 0x00 = Disabled (ITU default) 0x01 = Enabled (ANSI and Japan default)
0x03 | Not Used
0x04 | Network Indicator (NI) | 0x00=International 0x01=Reserved 0x02=National (default) 0x03=Reserved
0x05 | Reserved |
0x06 | Default SNM/SNT MSU Priority | 0x00 (ITU default) 0x03 (ANSI and Japan default)
0x07 | RCT MSU Priority | 0x00 = Dynamic (ANSI default) 0x01 = Static (non-ANSI) default
0x08 | ASP Restart Filtering | 0x00 = Disable (ANSI default) 0x01 = Enabled (non-ANSI default)
0x09 | SP Restart Filtering | 0x00 = Disable (ANSI default) 0x01 = Enabled (non-ANSI default)
0x0A | Reserved |
0x0B | Clear report counters/duration after reporting. | 0x00 disabled (default) 0x01 enabled
0x0C | Multi-host routing control. This byte affects all PPL Event Indications in this document. All previously existing PPL Event Indications are not affected. | 0x00 force routing to port 0x3142 0x01 force routing to port 0x3143 0x02 force routing to port 0x3144 0x03 force routing to port 0x3145 0x04 force routing to port 0x3146 0xFF force routing disabled (default)
0x0D | PPL Event Compatibility Mode. This byte affects previously existing PPL Event Indications to which the Q.752 Parameters ICB have been added. | 0x00=Q.752 Parameters Enabled (default) 0x01=Q.752 Parameters Disabled
0x0E | Reserved |
0x10 | Turn on/off SS7 MTP3 Message Tracing capability for HMRT. 1=On 0=Off | 0x00
| Raw MSU transmitted and received to and from the adjacent Node | 0x00=Disable (default) 0x01=Enable the PPL Event Indication containing the LSSU transmitted to the adjacent Node
0x11 | Reserved |
0x12 | Japan A/B plane insertion Setting this configuration byte to 0x01 enables the HMRT component to operate in a Japan DDI network. It enables the proper insertion of the link set using the A/B plane bit for COA and CBA Message Signaling Units when connected to a STP pair using a common point code. Setting this byte to 0x01 should only be used in the Japan DDI network, but not in the Japan JT and Japan NTT networks. This byte has no effect in non-Japan networks. | 0x00=Disabled (default) 0x01=Enabled
0x13 | ANSI bit rotation | 0x00 = Disabled (default for non-ANSI variants 0x01 = Enabled (default for ANSI variant)

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)
Signaling Point
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
See Signaling System Number Seven.
Message Transfer Part level 3 - network level