0x1E Generic PPL

This ICB is used in various scenarios including call routing and establishing IP calls.

Used in:

Route Control message
PPL Event Indication message
PPL Event Request message
Channel Release with Data message

ICB Type | 0x02 (Data)
ICB ID | 0x1E
Data Length | Total number of bytes below this line
Data[0, 1] | Total Number of TLVs
Data[2, 3] | TLV 1 Tag
Data[4, 5] | TLV 1 Length
Data[6] | TLV 1 Data[0]
Data[:] | :
Data[:] | TLV 1Data[n]
Data[2, 3] | TLV n Tag
Data[4, 5] | TLV n Length
Data[6] | TLV n Data[0]
Data[:] | :
Data[:] | TLV n Data[n]
TLVs | 0x01 Add Virtual Card 0x0009 Terminating Channel 0x000F Router Protocol ID 0x0013 Routing Method 0x0065 Physical VoIP Channel 0x0071 Virtual VoIP Channel 0x0100 RTP Payload Type (VDAC-ONE) 0x0100 RTP Payload Type (IPN Series 2) 0x0102 RTP Silence Suppression 0x0103 RTP Echo Cancellation 0x0116 Channel Service TLV 0x0117 Alerting Propagation Mode 0x0118 Companding Conversion Mode 0x0119 Media Offer Stage 0x011A Call Agent Mode Physical Channel ID 0x01C2 Minimum Jitter Buffer Delay 0x01C3 Maximum Jitter Buffer Delay (IPN-2 Card) 0x01C4 Adaptation Rate 0x01C5 Fax Type Enable 0x01C7 Fax/Modem Bypass Coder Type 0x01C8 Protocol Type 0x01D1 RTP Payload Redundancy 0x01D2 Fax Payload Redundancy 0x01D4 Type of Service 0x01DF UDP Source Port Validate 0x01E1 Fax Compatibility Mode 0x01E2 RFC 2833 Enable 0x01E6 Source T.38 Port 0x01E7 Destination T.38 Port 0x01E8 Source RTCP Port 0x01E9 Destination RTCP Port 0x01EB RTP Timer Timeout (VDAC-ONE) 0x01EC Media Inactivity Detection Timer 0x11 Signaling Route Test Control Status 0x12 Signaling Route Test Control DPC

See Information Control Block.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.