0x45 Child Conference ID

Use this AIB to create a Child Conference using the Resource Create message. The Child Conference ID should be set to 0xFFFF. The AIB in the response to the Resource Create message will contain the Parent Conference ID as well as the Child Conference ID, which is allocated by the CSP.

Use this AIB to connect to a Child Conference with the Resource Connect message. Indicate the actual Child Conference ID.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x45
3 | Data Length: 0x04
4, 5 | Data[0] Parent Conference ID
6, 7 | Data[1] Child Conference ID

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.