H.323

Comp. ID | Comp. Name | PPL Assign | PPL Audit Config. | PPL Audit | PPL Configure | PPL Data Query | PPL Event Request/ Indication | PPL Timer Config
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x00A0 | L3P RAS | Channel (0x0D) | N/A | Channel (0x0D)
0x00A1 | L3P H.225 | Channel (0x0D) | Channel (0x0D)
0x00A2 | L3P H.245 | Channel (0x0D) | Channel (0x0D)

Important! AIB (00 01 0d 03 ff ff ff) is valid for the following PPL Event Requests and Indications which are not related to any active calls: RRQ, URQ, RCF, UCF, RRQ FAIL, URQ FAIL, RRJ, URJ.
Other PPL Event Requests and Indications have a valid Span Channel.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
The Registration, Admission, and Status messages communicated between two H.323 entities for example between an Endpoint and a Gatekeeper.
See Address Information Block.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.