L3P BCC Protocol PPL Timers (0x008C)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Allocation Complete Wait | 1.5 seconds
0x02 | Deallocation Complete Wait | 2 seconds
0x03 | Deallocation Complete Wait (in Null state) | 2 seconds
0x04 | Audit Complete Wait | 1.5 seconds
0x05 | AN Fault Acknowledge Wait | 1.5 seconds
0x06 | Waiting for Datalink Connection Establish | 4 seconds

See Programmable Protocol Language.