You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Setting Ethernet Link Redundancy on a DSP Series 2 card

Setting Ethernet Link Redundancy on a DSP Series 2 card

You can provision and monitor the DSP Series 2 card ethernet redundancy options using the Converged Services Administrator.

The following topics relate to the card updates and ethernet link redundancy feature:

Querying Active Ethernet Interface 7-75

Enable Ethernet Redundancy 7-77

Disable Ethernet Redundancy 7-79

Performing an Ethernet Redundancy SwitchOver 7-81

Digital Signal Processor
CSA. GUI-based tool used to configure, provision and monitor a Excel platform related to, for example, SIP, H.323, and VDAC Resouce Attributes.