0x05F7 DSP Function Statistics

This TLV is included in the response to the Statistics Query message. It reports average free channels, minimum free channels, and total requests for each function on a specific DSP chip on a DSP module. This data is repeated for the Txmt0, Rcv0, Txmt1, and Rcv1.

Byte | Description
0, 1 | Tag:0x05F7 - DSP Function Statistics
2, 3 | Length: 0x000C
4 | Value[0]: Module Number 0x00 - DSP Module 0 0x01 - DSP Module 1
5 | Value[1]: Processor Number Valid Range - 0x00 - 0x03
6 | Value[2]: Sub-DSP Section 0x00 - Receive 0 0x01 - Transmit 0 0x02 - Receive 1 0x03 - Transmit 1
7 | Value[3]: Function Number
8-11 | Value[4-7]:Total Requests for Function
12, 13 | Value[8, 9]: Average Free Channels
14, 15 | Value[10, 11]: Minimum Free Channels

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor