You are here: CSP Developer’s Guide: Overview > 6 Layer 4 Call Control PPL Information > PPL Component for Interworking (0x0084)

PPL Component for Interworking (0x0084)

Configuration Bytes

The table below shows the PPL Configuration Byte values for the Layer 4 Interworking component

Byte (Hex) | Function | Values
--- | --- | ---
0x03 | Local Network Protocol ID | 0x01 - SS7
0x04 | Local Network Protocol Flavor | SS7 0x01 - ISUP ANSI 0x02 - ISUP ITU
0x0E | Host Protocol ID | 0x05 - Universal Protocol
0x0F | Host Protocol Flavor | 0x01 - Universal Flavor

See Programmable Protocol Language.
Call processing layer of the CSP.
Interworking is a software feature within the Excel platform call control layer that enables protocol conversion by analyzing and converting Network Signaling (NS) Layer 3 information.
See Signaling System Number Seven.
See Integrated Services Digital Network User Part.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.