You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > NGA Configure 0x0130

NGA Configure 0x0130

SwitchKit Name

NGAConfigure

Type

EXS and SwitchKit API message

Description

NGA Configure 0x0130

Configures the M3UA stack and objects.

Sent by

Host application

Related API Messages

NGA Service Configure (0x0160)
NGA Configure Query (0x0131)
NGA Service Query (0x0161)
NGA State Notify (0x0163)
NGA State Query (0x0162)

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_NGAConfigure;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE reserved6[13];

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[219];

} XL_NGAConfigureAck;

C++ Class

class XLC_NGAConfigure : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

}

C++ Class Response

class XLC_NGAConfigureAck : public

XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

; UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData();

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0130) | 3, 4 | Message Type (0x0130)
5, 6 | Sequence Number | 5, 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x03 - Item | 8, 9 |
10 | Checksum
Number of AEs to Follow
AEs 0x65 Global Object ID 0x67 Functional Area 0x08 SS7 Stack 0x64 Global Object Type
: | Data Type 0x00 - TLVs
: | Number of TLVs
: | 0xE001 Command
: | Data TLVs 0x9041 Protocol Parameters 0x9042 Application Server 0x9043 Application Server Process 0x9044 Signaling Gateway 0x9045 Signaling Gateway Process 0x9046 Connection 0x9052 Route Set 0x9053 Modify Destination
| Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.