You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > IP Signaling Series 3 Card Host Poll 0x0104

IP Signaling Series 3 Card Host Poll 0x0104

Type

EXS API message

Description

IP Signaling Series 3 Card Host Poll 0x0104

This message is sent unsolicited from the IP Signaling Series 3 card to the host on a periodic basis to allow the host to monitor the status of the IP Signaling Series 3 card. The default poll interval is one second.

Sent by

CSP

EXS Hex API Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x000B)
3, 4 | Message Type (0x0104) | 3, 4 | Message Type (0x0104)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | : | AIB Same as message
Number of AEs to follow
AEs 0x52 IP Signaling Series 3 Card ID or Expanded Logical Node ID 0x53 Object Type
: | Number of TLVs to Follow (0x01) | : | Checksum
: | TLV 0x0021 IP Signaling Series 3 Card Host Poll
: | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.