You are here: CSP Hardware Installation and Maintenance > 4 Card Installation > Card Types

Card Types

Overview

The cards used in the CSP (CSP 2090, CSP 2110 and CSP 2040) chassis are listed by card type below.

Important! Refer to each cards Hardware Product Description for specific illustrations, compliance, LED descriptions, switch settings, jumper settings, model numbers, and part numbers.

Power Supply Cards

These are the currently available Power Supply cards.

PSC-150 Power card (CSP 2090 and CSP 2110)

PSC-60 Power card (CSP 2040)

CSP Matrix Controller Series 3 Cards

These are the currently available CSP Matrix Controller Series 3 cards.

CSP Matrix Controller Series 3 card

CSP Matrix Controller Series 3 I/O card

Line Cards

These are the currently available Line cards.

DS3 card

DS3 I/O card

DS3 Standby I/O card

E-ONE card

E-ONE 120 Ohm I/O card

E-ONE 120 Ohm Redundant I/O card

E-ONE 120 Ohm Standby I/O card

E-ONE 75 Ohm I/O card

E-ONE 75 Ohm Redundant I/O card

E-ONE 75 Ohm Standby I/O card

J-ONE card

J-ONE Redundant I/O card

J-ONE Standby I/O card

T-ONE card

T-ONE 100 Ohm I/O card

T-ONE 100 Ohm Redundant I/O card

T-ONE 100 Ohm Standby I/O card

Common Channel Signaling (CCS) Cards

These are the currently available CCS cards.

CCS I/O card

CCS I/O Series 3 car d

ISDN PRI card

ISDN PRI Redundant I/O card

ISDN Series 3 card (The CCS I/O Series 3 card is the I/O card for this card.)

SS7 PQ card (The CCS I/O card is the I/O card for this card.)

SS7 Series 3 card (The CCS I/O Series 3 card is the I/O card for this card.)

Resource Cards

These are the currently available Resource cards.

DSP-ONE card

Subrate Controller card

DSP Series 2 card

DSP Series 2 Plus card

EXNETฎ Cards

The following is currently the available EXNETฎ cards.

EXNET-ONE car d

Important! EXNET Connectฎ PCI H.100 card The EXNET Connect PCI H.100 card is not supported in Release 8.4.1. Refer to the CSP Technical Publication for Release 8.3.1 for information on this card.

Internet Protocol (IP) Cards

These are the currently available IP cards.

IP Signaling Series 3 card (The CCS I/O Series 3 card is the I/O card for this card.)

VDAC-ONE card

VDAC I/O card

IP Network Interface Series 2 card

Multi-Function Media I/O card

IP Network Interface Series 3 card

Blockout Cards and Panels

Install blockout cards in unoccupied card slots to improve air flow and cooling. Use blockout cards in any unoccupied slot both in front and rear of the CSP chassis.

The Matrix Controller Series 3 card is based on Motorolas 750 PowerPC processor (68750). It is often referred to as the Matrix Controller.
CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
See Common Channel Signaling.
See Integrated Services Digital Network.
See Signaling System Number Seven.
Digital Signal Processor
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
Peripheral Component Interconnect
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.