0x05E8 Beep Tone Parameters

Use this TLV in the Record File Start message to enable Beep Tone, as well as its frequency, duration, and amplitude.

Byte | Description
0, 1 | Tag 0x05E8 Beep Tone Parameters
2, 3 | Length 0x0005
4 | Value[0] Beep Enable Flag 0 Disable 1 Enable (Default)
5, 6 | Value[1, 2] Beep Frequency (Hz) Minimum 100 (0x0064) Maximum 3000 (0x0BB8) Default 1000 (0x03E8)
7 | Value[3] Beep Duration (10 ms steps) Minimum 3 (0x03) Maximum 200 (0xC8) Default 20 (0x14)
8 | Value[4] Beep Amplitude, in decibel milliwatts (dBM) Minimum -54 (0xCA) Maximum 3 (0x03) Default -15 (0xF1)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Message delimiter (SS7 bit pattern - 01111110)
Hertz