You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Node Status Query 0x006F

Node Status Query 0x006F

SwitchKit Name

NodeStatusQuery

Type

EXS API and SwitchKit API message

Description

Node Status Query 0x006F

Use this message to query the status of a CSP node in a multi-node system. The status is reported in the response.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

} XL_NodeStatusQuery;

C Structure Response

typedef struct {

unsigned short Status;

int PhysicalNode;

UBYTE LogicalNode;

UBYTE HostNode;

UBYTE NodeStatus;

} XL_NodeStatusQueryAck;

C++ Class

class XLC_NodeStatusQuery : public XLC_OutboundMessage {

public:

};

C++ Class Response

class XLC_NodeStatusQueryAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

int getPhysicalNode() const;

void setPhysicalNode(int x);

UBYTE getLogicalNode() const;

void setLogicalNode(UBYTE x);

UBYTE getHostNode() const;

void setHostNode(UBYTE x);

UBYTE getNodeStatus() const;

void setNodeStatus(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x006F) | 3, 4 | Message Type (0x006F)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
| Number of AEs to follow
| AE
: | Checksum | 10 | AIB Same as message
: | Host Node ID The value here is the same as the Logical Node ID field in the header. The system uses the value 0xF0 for a host node that does not have a logical node ID.
: | Node Status This field indicates the current status of the node. 0x00 Node Initialized 0x01 Reassigning Host Node – A new host is indicated in the Host Node field 0x04 Multi Node System – ISUP Remote Control 0xFF Node Requires Logical Node ID
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
See Integrated Services Digital Network User Part.