0x0034 LAPD Frame

Used in:
PPL Event Request message
PPL Event Indications message

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0034
Data Length (2 bytes) | Length of Layer 3 Information
First Byte of Layer 3 Data | Variable
: |
Last Byte of Layer 3 Data | Variable

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
Protocol layer of the CSP.