You are here: CSP Hardware Product Descriptions > 1 Chassis > CSP 2090 Fan Tray, Rear - LNXFTR1000/LNXFTR1000R

CSP 2090 Fan Tray, Rear - LNX-FTR-1000/LNX-FTR-1000R

Description

The rear fan tray and front fan tray, as shown below, are both required to ensure proper air flow and cooling of the CSP 2090 chassis. The rear fan tray is powered by the -48 V DC midplane bus. It can be removed with the power ON. The rear fan tray does not have an air filter, it is maintenance-free.

Refer to the Hardware Installation and Maintenance Guide to access the rear fan tray.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the fan tray.

Specifications

The rear fan tray is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Input Power Requirement | -48 V DC
Input Voltage Range | -40 V DC to -60 V DC

Physical | Specification
--- | ---
Height | 7.2 cm (2.85 in.)
Width | 43.5 (17 in.)
Depth | 21.0 cm (12.5 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the CSP 2090 rear fan tray are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
CSP 2090 Chassis | EXS-CHA-1100 | EXS-CHA-1100R

Fan Tray Locations

This drawing shows the location of the fan trays.