You are here: CSP API Reference > 3 Information Control Blocks > SS7 and ISDN Values

SS7 and ISDN Values

This section provides data values required for SS7 ICBs, including the following:

• SS7 Parameter IDs

• MTP Statistics Parameter IDs from Q.752

See "SS7 ISUP Message Format Configure 0x6B" for a list of ISUP Message IDs.

In this section:

SS7 Parameter IDs

MTP Parameter IDs from Q.752

ISDN Values

Information Elements

0x01 Call Reference

0x02 Called Party Number

0x03 Calling Party Number

0x04 Called Party Subaddress

0x05 Calling Party Subaddress

0x06 Redirecting Number

0x07 Cause

0x08 Progress Indicator

0x09 User-to-User

0x0A Codeset 6

0x0B Codeset 7

0x11 Codeset 5

0x12 Vari-A-Bill

0x13 Directory Number (DN) Provisioning

V5 Information Elements

V5 PSTN IEs

0x01 Pulse Notification

0x02 Line Information

0x03 State

0x04 Autonomous Signaling Sequence

0x05 Sequence Response

0x06 Reserved

0x07 Cadence Ringing

0x08 Pulsed Signal

0x09 Steady Signal

0x0A Digit Signal

0x0B Recognition Time

0x0C Pulsed Signal

0x0D Disable Autonomous Acknowledge

0x0E Cause

0x0F Cause

Parameter Type Values for Cadence Ringing Extended IE

0x10 Cadence Ringing Extended (Type A - Digits and Characters Present)

0x10 Cadence Ringing Extended (Type B - Digits Present, Characters Missing )

0x10 Cadence Ringing Extended (Type C - Digits Missing, Characters Present)

0x10 Cadence Ringing Extended (Type D - Digits and Characters Missing)

0x11 Reserved

0x12 Called Party

V5 BCC IEs

0x15 User Port ID IE

0x17 V5 Timeslot ID IE

0x1B V5 Timeslot ID IE

IE Fields

Billing Type

Coding Standard

Location

Number Plan Identification

Presentation Indicator

Progress Indicator

Reason For Redirection

Recommendation

Screening Indicator

Type of Number

Cause Codes

See Signaling System Number Seven.
See Message Transfer Part.
See Integrated Services Digital Network User Part.