L3 BT IUP CPC PPL Event Indications

Event ID | Event
--- | ---
0x01F5 | Invalid IFAM message received from the Network
0x01F6 | Invalid SAM message received from the Network
0x01F7 | Invalid FAM message received from the Network
0x01F8 | Invalid IAM message received from the Network
0x01F9 | Invalid ASUI message received from the Network
0x01FA | Invalid SND message received from the Network
0x01FB | Invalid SAD message received from the Network
0x01FC | Invalid SASUI message received from the Network
0x01FD | Invalid ACM message received from the Network
0x01FE | Invalid CNG message received from the Network
0x01FF | Invalid CNA message received from the Network
0x0200 | Invalid RAM message received from the Network
0x0201 | Invalid ANS message received from the Network
0x0202 | Invalid CLR message received from the Network
0x0203 | Invalid REL message received from the Network
0x0204 | Invalid CCF message received from the Network
0x0205 | Invalid BLO message received from the Network
0x0206 | Invalid UBL message received from the Network
0x0207 | Invalid BLA message received from the Network
0x0208 | Invalid UBA message received from the Network
0x0209 | Invalid CFN message received from the Network
0x020A | Invalid ACI message received from the Network
0x020B | Invalid SEM message received from the Network
0x020C | Invalid TLV Length
0x020D | Invalid Number of TLVs
0x020E | Glare Indication Caused by IAM
0x020F | Glare Indication Caused by IFAM
0x0210 | Invalid SOO message received from the Network
0x0212 | Invalid SER message received from the Network
0x0213 | Invalid SIM message received from the Network
0x0214 | Invalid OOR message received from the Network
0x0215 | Invalid HLR message received from the Network
0x0216 | Invalid SSM message received from the Network
0x0217 | Invalid CFC message received from the Network
0x0218 | Invalid ECM message received from the Network
0x0219 | Invalid OLM message received from the Network
0x021A | Invalid SUS message received from the Network
0x021B | Invalid RES message received from the Network
0x021C | Invalid SWAP message received from the Network
0x021D | Non-receipt of CFC or BLO has occurred
0x021E | Invalid RAN message received from the Network
0x021F | Invalid TCM message received from the Network

Random Access Memory
Blocking Acknowldgment message
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Recorded Announcements.