You are here: SwitchKit® Development Environment Programmer’s Guide > 1 SwitchKit® Application Programming Interface > API Messages Used for Call Control Programming

API Messages Used for Call Control Programming

This section outlines the messages used for developing call control applications.

Call Control

BusyOut
CallProcessingEvent
CPAResult
ChannelReleased
ChannelReleasedWithData
ChannelReleaseRequest
CollectDigitString
ConferenceCreate
ConferenceDeleted
ConferenceDeleteRequest
Connect
ConnectOneWayForced
ConnectOneWayToConference
ConnectToConference
ConnectTonePattern
ConnectWait
ConnectWithData
ConnectWithPad
CPCDetection
CrossConnectChannel
CrossConnectSpan
CrossDisconnectChannel
CrossDisconnectSpan
DisconnectTonePattern
DS0StatusChange
DSPCacheModify
DSPServiceCancel
DSPServiceRequest
GenerateCallProcessingEvent
InseizeControl
OutpulseDigits
OutseizeControl
ParkChannel
PlayFileModify
PlayFileStart
PlayFileStop
PPLEventIndication
PPLEventRequest
RecAnnConnect
RecAnnDelete
RecAnnDisconnect
RecAnnDownload
RecAnnDownloadInit
RecordFileModify
RecAnnFSConvert
RecAnnFSDefrag
RecAnnSingleDelete
RecordFileModify
RecordFileStart
RecordFileStop
ReleaseChannel
ReleaseWithData
Remove Channels From Group
Request For Service
ResourceConnect
Resource Create
ResourceDelete
Resource Modify
RFSWithData
Route Control

Setting up, monitoring, and tearing down calls.
RFS. A Status Message indicating that some entity is requesting service from the Excel platform.