You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > AddSS7TCAPCard

AddSS7TCAPCard

Type

EXS SwitchKit API message

Overview

The AddSS7TCAPCard message is used to make a direct TCP connection between the LLC Host and a SS7 card for the purpose of routing TCAP traffic on a separate link. This message creates the appropriate AddLLCCard messages and sends them to the LLC.

Sent by

Host, using Converged Services Administrator (CSA), webCSA or SwitchManager configuration file.

Arguments

The following table shows the arguments that you can modify:

Argument | Description
--- | ---
CardIP1 | The primary SS7 card IP address in the CSP.
CardIP2 | The standby SS7 card IP address, if it exists. If there is only one SS7 card in the node, this field should be set to "", that is, the 0-length string.
StackID | The ID of the TCAP stack to which the LLC connects.
SSN | The Subsystem Number configured on the SS7 card to which the LLC should connect.
ControlNode | The logical node ID assigned to the CSP Matrix Series 3 Card which controls the chassis where the SS7 card resides.
Action | 0x00 To add a connection 0x01 To remove a connection and all RoutingIDs

C Structure

typedef struct {

char CardIP1[30];

char CardIP2[30];

UBYTE StackID;

UBYTE SSN;

int ControlNode;

UBYTE Action;

UBYTE reserved84[5];

} SK_AddSS7TCAPCard;

C++ Class

class SKC_AddSS7TCAPCard : public SKC_DummyMessage {

public:

const char *getCardIP1() const;

void setCardIP1(const char *x);

const char *getCardIP2() const;

void setCardIP2(const char *x);

UBYTE getStackID() const;

void setStackID(UBYTE x);

UBYTE getSSN() const;

void setSSN(UBYTE x);

int getControlNode() const;

void setControlNode(int x);

UBYTE getAction() const;

void setAction(UBYTE x);

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Signaling System Number Seven.
See Transaction Capability Application Part.
CSA. GUI-based tool used to configure, provision and monitor a Excel platform related to, for example, SIP, H.323, and VDAC Resouce Attributes.
See Converged Services Administrator.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.