You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > SwitchBackFromStandby

SwitchBackFromStandby

Type

SwitchKit API message

Description

Use the SK_SwitchBackFromStandby message to initiate a switchback from a standby line card to the primary one. This message can only be sent if the action field of the message SK_SwitchBackFromStandbyConfig is set to 1 during configuration.

Sent by

Application or Converged Services Administrator (CSA).

Arguments

The following table shows the arguments that you can modify:

Argument | Description
--- | ---
Action | This field can be set to: • 0 = graceful switchback after LLC determines that the standby card is not handling any calls. • 1 = forced switchback immediately.
Node | Specifies the node where the switchback is supposed to happen.
StandbySlot | Specifies the standby slot of the redundant card.

C Structure

typedef struct {

UBYTE StandbySlot;

UBYTE Action;

} SK_SwitchBackFromStandby;

C Structure Response

typedef struct {

int Status;

} SK_SwitchBackFromStandbyAck;

C++ Class

class SKC_SwitchBackFromStandby : public SKC_ToolkitMessage {

public:

UBYTE getStandbySlot() const;

void setStandbySlot(UBYTE x);

UBYTE getAction() const;

void setAction(UBYTE x);

};

C++ Class Response

class SKC_SwitchBackFromStandbyAck : public SKC_ToolkitAck {

public:

int getStatus() const;

void setStatus(int x);

};

CSA. GUI-based tool used to configure, provision and monitor a Excel platform related to, for example, SIP, H.323, and VDAC Resouce Attributes.
See Converged Services Administrator.