You are here: PPL Developer’s Guide > 7 ISDN Atomic Functions > L3P MGR (0x0093) Atomic Functions

L3P MGR (0x0093) Atomic Functions

This section describes the atomic functions for the L3P MGR PPL component.

L3P MGR Atomic Functions

The following atomic functions are specific to the ISDN MGR PPL component.

AF Number | 51
Name | Query All Span Status
Description | This function queries All Span Status
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 52
Name | Check whether all spans are alive
Description | This function checks whether all spans are alive
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | PPL Int Event 1 = Success; PPL Int Event 0 = Failure

AF Number | 53
Name | Update the Layer 3P L Manager Link Status
Description | This function updates the Layer 3P L Manager Link Status
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 54
Name | Configure general for Envelope Function Layer
Description | This function configures general for Envelope Function Layer
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 55
Name | Configure general for LAPV
Description | This function configures general for LAPV
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 56
Name | Configure general for L3
Description | This function configures general for L3
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 57
Name | ConfigureV5 Interface
Description | This function configuresV5 Interface
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 58
Name | Configure User Ports
Description | This function configures User Ports
Arg1 | 0 = Configure User Ports; 1 = Add User Ports
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 59
Name | Set Don’t do General Configuration Global Data Variable
Description | Function sets Don’t do General Configuration Global Data Variable
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 60
Name | Clear Don’t do General Configuration Global Data Variable
Description | Function clears Don’t do General Configuration Global Data Variable
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 61
Name | Check Don’t do General Configuration Global Data Variable
Description | Function checks Don’t do General Configuration Global Data Variable
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | PPL Int Event 1 = Set; PPL Int Event 0 = Not Set

AF Number | 71
Name | Send Startup Request to System Management
Description | This function sends Startup Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 72
Name | Send Startup Event PPL Event Indication to host <Arg1>
Description | This function sends Startup Event PPL Event Indication to host
Arg1 | Any one of the following: 1: Startup Layer-2 Activation Fail 2: Startup Variant ID Mismatch 3: Startup Link ID Failed 4: Startup Complete 5: Startup Failed
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 73
Name | Send Delete V5 Interface message to System Management
Description | This function sends Delete V5 Interface message to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 74
Name | Send V5 Interface Restart Request to System Management
Description | Sends V5 Interface Restart Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 75
Name | Send Restart Event PPL Indication to host <Arg 1>
Description | Sends V5 Interface Restart Request to System Management
Arg1 | 1 = Restart timer expired, Restart failed; 2 = Restart complete
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 76
Name | Send V5 Interface Status to host
Description | Sends V5 Interface Status to host
Arg1 | 0 = Interface is not up; 1 = Interface ID up
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 77
Name | Set the interface State
Description | Sets the interface State
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 78
Name | Print Interface Alive message
Description | Prints Interface Alive message
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 81
Name | Send Link Not in Operation message to System Management
Description | Sends Link Not in Operation message to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 82
Name | Send Blocked Link Indication to System Management
Description | Sends Blocked Link Indication to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 83
Name | Send Deferred Link Block Request to System Management
Description | Sends Deferred Link Block Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 84
Name | Send Non-Deferred Link Block Request to System Management
Description | Sends Non-Deferred Link Block Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 85
Name | Send Unblock Link Request to System Management
Description | Sends Unblock Link Request to System Management
Arg1 | 0 = Use the current Link 1 = Use other Link (Useful only with Primary and Secondary links, such as when Primary Link is blocked and Secondary C-Channel is active. For switchover when the current link is Secondary, this option sends a Link Unblock message to the Primary link.
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 86
Name | Send Link in Operation message to System Management
Description | Sends Link in Operation message to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 87
Name | Send Add Link Request to System Management
Description | Sends Add Link Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 88
Name | Send Delete Link Request to System Management
Description | Sends Delete Link Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 89
Name | Send Block Indication to System Management from timer expiry
Description | Sends Block Indication to System Management from timer expiry
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 90
Name | Send Link MDU PPL Event Indication to host <Arg1>
Description | Sends Link MDU PPL Event Indication to host
Arg1 | Any one of the following: 1 Link operational 2 Link not operational 3 Link ID Required 4 Link ID Request 5 Link ID Release Indication 6 Link ID Reject Indication 7 Link ID Failure 8 Link Block Indication 9 Link Unblock Indication 10 Link Unblock Request 11 Link Deferred Block Request 12 Link No-deferred Block Request
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 91
Name | Send Data Link Release Event PPL Event Indication to host <Arg1>
Description | This function sends Data Link Release Event PPL Event Indication to host
Arg1 | Any one of the following: 1: Data link release received, autonomous switchover initiated 2: Datalink down Indication, standby not configured 3: Data link release received, autonomous switchover to be initiated on getting control protocol DL release 4: BCC DL release, audit connection requested.
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 92
Name | Send Link Status to host
Description | Sends Link Status to host
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 93
Name | Send Layer 3P PSTN Link Blocked Request
Description | Sends Layer 3P PSTN Link Blocked Request
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 94
Name | Send Link Down message to Layer 3P PSTN
Description | Sends Link Down message to Layer 3P PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 95
Name | Send Deferred Link Block Request to Layer 3P PSTN
Description | Sends Deferred Link Block Request to Layer 3P PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 96
Name | Send Non-Deferred Link Block Request to Layer 3P PSTN
Description | Sends Non-Deferred Link Block Request to Layer 3P PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 97
Name | Send User Port message to Layer 3P PSTN
Description | Sends User Port message to Layer 3P PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 99
Name | Send Channel Status to Layer 4 for all timeslots
Description | Sends Channel Status to Layer 4 for all timeslots
Arg1 | 0 = Channel Out Of Service 1 = Channel In Service 2 = Channel Blocked 3 = Clear Channel
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 100
Name | Set Link Status
Description | Sets Link Status
Arg1 | Value
Arg2 | Bit Mask
Returns | Success or Failure

AF Number | 101
Name | Return C Channel Status to Link
Description | Returns C Channel Status to Links
Arg1 | Value
Arg2 | Bit Mask
Returns | Success or Failure

AF Number | 102
Name | Check Primary or Secondary Link Up
Description | Checks Primary or Secondary Link Up
Arg1 | Value
Arg2 | Bit Mask
Returns | Success or Failure

AF Number | 103
Name | Test Link Status
Description | Tests Link Status
Arg1 | Bit Mask
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 104
Name | Send all configured links status to System Management
Description | Sends all configured links status to System Management
Arg1 | 0 = Block only locally-blocked Links 1 = Unblock Unblocked Links
Arg2 | Bit Mask
Returns | Success or Failure

AF Number | 105
Name | Send MPH AIs to System Management
Description | Sends MPH AIs to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 111
Name | Check whether other C Channel is active
Description | Checks whether other C Channel is active (other than the channel that is currently active)
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 112
Name | Send C Channel Status to host
Description | Sends C Channel Status to host
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 113
Name | Send Accelerated Port Alignment Request to System Management
Description | Sends Accelerated Port Alignment Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 114
Name | Send User Port Block Request to System Management
Description | Sends User Port Block Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 115
Name | Send User Port Unblock Request to System Management
Description | Sends User Port Unblock Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 116
Name | Send User Port Block Indication to System Management
Description | Sends User Port Block Indication to System Management
Arg1 | 0 = Send Block Indication 1 = Send Don’t Locally block Indication
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 117
Name | Send Delete User Port message to System Management
Description | Sends Delete User Port message to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 118
Name | Send User Port Status Request to System Management
Description | Sends User Port Status Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 119
Name | Send MPH PPL Event Indication to host <Arg1>
Description | Sends MPH PPL Event Indication to host
Arg1 | Any one of the following: 1 Port Unblock Request 2 Port Block Indication 3 Port Unblock Indication 4 Port Block Request 5 ISDN-PRI AN Maintenance 6 ISDN-PRI AN Maintenance 7 ISDN-PRI AN Maintenance 8 ISDN-PRI AN Maintenance 9 ISDN-PRI AN Maintenance 10 ISDN-PRI AN Maintenance 11 ISDN-PRI AN Maintenance 12 ISDN-block D-channel from user 13 ISDN Unblock D-channel 14 User Failure Indication from Userport 15 Network failure indication 16 Access Activated 17 Access Deactivated 18 Grading Information 19 Reception of FE2 20 DS Active 21 Indication of DL Failure 22 Indication of LOS/LFA 23 Reception of FE101 24 Reception of FE105 25 Unsuccessful Activation Attempt 26 Access Activation by User
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 120
Name | Send Userport Status to host
Description | Sends Userport Status to host
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 121
Name | Send Port Error PPL Event Indication to host <Arg 1>
Description | Sends Port Error PPL Event Indication to host
Arg1 | 1 = Port FSM received an invalid Event
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 122
Name | Test whether call is active on the Userport
Description | Tests whether call is active on the Userport or not
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 123
Name | Send Block Indications to System Management for the ports that are locally blocked
Description | Sends Block Indications to System Management for the ports that are locally blocked
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 124
Name | Send Unblock Request to System Management for all ports, then send Block Indications to ports that are locally blocked
Description | Sends Unblock Request to System Management for all ports, then send Block Indications to ports that are locally blocked
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 131
Name | Send Switchover Request to System Management
Description | Sends Switchover Request to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 132
Name | Send Switchover Complete message to System Management
Description | Sends Switchover Complete message to System Management
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 133
Name | Send Switchover Event PPL Indication to host <Arg 1>
Description | Sends Switchover Event PPL Indication to host
Arg1 | Any of these: 1 = Layer Manager to perform Envelope function layer SAP config. 2 = Switchover reject received 3 = Switchover completed 4 = Switchover failed
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 134
Name | Send Reconfigure to Ev Layer for Switchover
Description | Sends Reconfigure to Ev Layer for Switchover
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 135
Name | Straighten out Ev SAPs
Description | Straightens out Ev SAPs
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 136
Name | Test whether Ev crossed
Description | Tests whether Ev crossed
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 137
Name | Toggle Ev SAPs
Description | Toggles Ev SAPs
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 138
Name | Check for reasons for switchover fail
Description | Checks for reasons for switchover fail. Returns 0 (indicating failure) in any of these cases: Both C-Channels are Dead Both C-Channels are blocked One C-Channel is Dead and the other is blocked
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 141
Name | Send Statistics Error PPL Event Indication to host <Arg 1>
Description | Sends Statistics Error PPL Event Indication to host <Arg 1>
Arg1 | 1 = Invalid Entity, Instance 2 = Invalid Port ID
Arg2 | <Not Used>
Returns | PPL Int Event 1 (Success); PPL Int Event 0 (Failure)

AF Number | 142
Name | Send Statistics request to lower layers
Description | Sends Statistics request to lower layers (System Management, Envelope layer, or LAPV)
Arg1 | 1 = Invalid Entity, Instance 2 = Invalid Port ID
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 143
Name | Send Statistics data to host
Description | Sends Statistics data to host
Arg1 | 0 = Vf Layer Statistics 1 = Ev layer Statistics 2 = LAPV Statistics
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 146
Name | Send Status Indication to Layer 3P BCC
Description | Sends Status Indication to Layer 3P BCC
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 147
Name | Send Status Error PPL Event Indication to host <arg1>
Description | This function sends Status Error PPL Event Indication to host
Arg1 | Any of the following: 1 Invalid entity and Instance 2 Invalid Interface Number 3 Invalid port type 4 Invalid port ID 5 Invalid Link number
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 149
Name | Process the LAPV Status Indication
Description | Processes the LAPV Status Indication
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 151
Name | Set HDLC Driver Action
Description | Sets HDLC Driver Action
Arg1 | 0 = Disable 1 = Enable 2 = Disable All
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 152
Name | Disable HDLC Driver for blocked or dead C Channels
Description | Disables HDLC Driver for blocked or dead C Channels
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 153
Name | V5 MGR test whether V5 Subscriber ID exists
Description | Tests whether V5 Subscriber ID exists
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 154
Name | V5 MGR send PPL Event Indication to Layer 5 with V5 Subscriber ID
Description | Sends PPL Event Indication to Layer 5 with V5 Subscriber ID
Arg1 | Ev Indication
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 155
Name | V5 MGR send PPL Event Indication to Layer 5 with no ICB
Description | V5 MGR sends PPL Event Indication to Layer 5 with no ICB
Arg1 | Event Indication Number
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 161
Name | Send Management Port PPL Event Indication to host <Arg 1>
Description | Sends Management Port PPL Event Indication to host
Arg1 | 1 = Event out of sequence 2 = Saved Event already reached limit 3 = Timer T2 expired twice
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 162
Name | Send Management Common PPL Event Indication to host <Arg 1>
Description | Sends Management Common PPL Event Indication to host
Arg1 | 1 = Event out of sequence 2 = Saved Event already reached limit 3 = Timer T2 expired twice
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 163
Name | Send Event Message Decode PPL Indication to host <Arg 1>
Description | Sends Event Message Decode PPL Event Indication to host
Arg1 | 1 = Message Decoding Error 2 = Invalid message 3 = Invalid message length 4 = Protocol discriminator error 5 = Layer 3 address error 6 = Invalid message type 7 = Invalid message content 8 = Invalid optional IE
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 164
Name | Send Control Request OK PPL Event Indication to host <Arg1>
Description | This function sends Control Request OK PPL Event Indication to host
Arg1 | Any one of the following: 1: All Ports Blocked 2: All Linked Blocked 3: Port/All Port Deleted 4: Interface Deleted 5: Accelerated Port Alignment OK 6: All Links/Link Deleted
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 165
Name | Send Config OK PPL Event Indication to host
Description | This function sends Config OK PPL Event Indication to host
Arg1 | 1: V5 General CFG OK 2: V5 TSAP CFG OK 3: V5 Interface CFG OK 4: V5 Link CFG OK 5: V5 Userport CFG OK
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 166
Name | Send Acknowledgment to host in response to PPL Event Request
Description | Sends Acknowledgment to host in response to PPL Event Request
Arg1 | 0 = Positive Acknowledgment 1 = Invalid Event
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 168
Name | Send Layer 4 Primitive Failed PPL Event Indication to host
Description | Sends Layer 4 Primitive Failed PPL Event Indication to host
Arg1 | 0 = Reasons Available 1 = Reasons Unavailable
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 169
Name | Send Status Indication to Layer 3P PSTN
Description | Sends Status Indication to Layer 3P PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 170
Name | Send Invalid State PPL Event Indication to host <Arg1>
Description | Sends Invalid State PPL Event Indication to host
Arg1 | 1 = BCC/Protection protocol State event matrix received invalid event
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 171
Name | Send UI Event PPL Event Indication to host <Arg1>
Description | Sends UI Event PPL Event Indication to host
Arg1 | 1 = Layer 4 primitive failed, requested TSAP not found
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 172
Name | Send LVT INT Down PPL Event Indication to host <Arg1>
Description | Sends LVT INT Down PPL Event Indication to host
Arg1 | 1 = Control Protocol TCON Timer expired
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 173
Name | Send Common Event PPL Event Indication to host <Arg1>
Description | Sends Common Event PPL Event Indication to host
Arg1 | 1 = Ready for Reprovisioning 2 = Not ready for reprovisioning 3 = Variant and ID received 4 = Switchover to new variant 5 = Cannot reprovision 6 = Verify reprovisioning 7 = reprovisioning started
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 174
Name | Send message Send PPL Event Indication to host <Arg1>
Description | Sends message Send PPL Event Indication to host
Arg1 | 1 = Message send failure, Invalid protocol FSM State 2 = Protection protocol message send failure, both DLs down
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 175
Name | Send message Received PPL Event Indication to host <Arg1>b
Description | Sends message Received PPL Event Indication to host
Arg1 | 1 = Message received an Invalid protocol FSM State
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 176
Name | Send timer expired PPL Event Indication to host <Arg1>
Description | Sends timer expired PPL Event Indication to host
Arg1 | 1= Secondary expiry of Link control protocol timer
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 177
Name | Send L1 FSM PPL Event Indication to host <Arg1>
Description | This function sends L1 FSM PPL Event Indication to host
Arg1 | Any one of the following: 1: Layer Manager should issue MPH ID to Layer 1 2: Layer Manager should issue MPH IDR to Layer 1 3: Layer Manager should issue MPH NOR to Layer 1
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 178
Name | Send DSFE PPL Event Indication to host <Arg1>
Description | Sends DSFE PPL Event Indication to host
Arg1 | Any one of the following: 1: ISDN activate access 2: ISDN deactivate access
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 179
Name | Send Timer PPL Event Indication to host <Arg1>
Description | This function sends Timer PPL Event Indication to host
Arg1 | Any one of the following: 1: PSTN Timer T3 expiry 2: PSTN Timer T4 expiry
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 180
Name | Send Protection Layer PPL Event Indication to host <Arg1>
Description | This function sends Protection Layer PPL Event Indication to host
Arg1 | Any one of the following: 1: Reset SN error 2: General protocol error message 3: Notification to layer management of SN misalignment. 4: Reset SN Indication after action on reset SN Request 5: Reset SN acknowledge reception Indication
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 181
Name | Send Protocol Error Message PPL Event Indication to host <Arg1>
Description | This function sends Protocol Error Message PPL Event Indication to host
Arg1 | 1 = BCC Protocol Error message received
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 182
Name | Send Configuration Error PPL Event Indication to host <Arg1>
Description | This function sends Configuration Error PPL Event Indication to host
Arg1 | Any one of the following: 1 Invalid Entity, Instance 2 Invalid Element Type 3 Configuration already done 4 Cannot Allocate Memory 5 Invalid Interface Number 6 Link Already Present 7 Maximum links already present 8 Invalid Port Type 9 Ports exceed maximum ports 10 Port already present 11 Port insert into hash list failed
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 183
Name | Send Control Error PPL Event Indication to host <Arg1>
Description | This function sends Control Error PPL Event Indication to host
Arg1 | Any one of the following: 1 Invalid Entity, Instance 2 Invalid Interface number 3 Invalid Element, Type 4 Invalid unsolicited action 5 Invalid trace generation action 6 Invalid sub-action parameter 7 Block port error 8 Delete port error 9 Delete interface error 10 Delete link error 11 Invalid port ID 12 Block Link error
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 184
Name | Send Bind error PPL Event Indication to host <Arg1>
Description | This function sends Bind error PPL Event Indication to host
Arg1 | 1 = Layer 4 unable to bind/unbind to Layer 3
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 185
Name | Send Common Error PPL Event Indication to host <Arg1>
Description | This function sends Common Error PPL Event Indication to host
Arg1 | Any one of the following: 1: V5.1FSM getting a bad input event 2: Variant and ID-mismatch 3: V5.1FSM reporting control protocol DL failure 4: V5.1 FSM timer expiry 5: V5.2 interface FSM receiving bad Input event. 6: Accelerated port Alignment failed.
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 191
Name | Check whether LE Side
Description | Checks whether LE side
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 201
Name | Sec C Channel to change the State to Alive from Active
Description | Allows the Sec C Channel to change state to Alive from Active only when the primary C Channel is already active, and also to set both the C Channel states appropriately
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

See Programmable Protocol Language.
See Integrated Services Digital Network.
See Atomic Function.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Public Switched Telephone Network
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Call processing layer of the CSP.
Signaling technique where the full channel bandwidth is used for data transmission, while the framing and control bits (signaling) use a separate channel. No control or signaling is performed on this path. See B8ZS and ZBTSI.
Application layer of the CSP.
See Information Control Block.
Protocol layer of the CSP.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
Digital communications link - 44.378 Mbps rate