MTP3 HMDT Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | Variant | 0x00=ANSI 0x01=ITU 0x02=Japan TTC/DDI 0x03=China 0x04 = Japan NTT
0x02 | Reserved |
0x03 | Reserved |
0x04 | Network Indicator (NI) | 0x00=International 0x01=Reserved 0x02=National (default) 0x03=Reserved
0x05 | Not used |
0x06 | ANSI Cluster Fanout | 0x00 = Disabled (default for all variants except ANSI) 0x01 = Enabled (default for ANSI variant)
0x07 | TRW SNM MSU | 0x00 = Disabled (default for all variants except ANSI) 0x01 = Enabled (default for ANSI variant)
0x08 to 0x0B | Reserved |
0x0C | Multiple network congestion states | 0x00 = Disabled (default for all variants except ANSI and Japan) 0x01 = Enabled (default for ANSI and Japan variants)
0x0D | UPU unavailability cause | 0x00 = Disabled (default for ANSI variant) 0x01 = Enabled (default for all variants except ANSI)
0x0E to 0x0F | Reserved |
0x10 | Turn on/off SS7 MTP3 Message Tracing capability for HMDT | 0=Off (default) 1=On
| Raw MSU transmitted and received to and from the adjacent Node | 0x00=Disable (default) 0x01=Enable the PPL Event Indication containing the LSSU transmitted to the adjacent Node
0x11 | TUP Selector | 0x00 = TUP (default) 0x01 = BT-IUP
0x12 | Japan A/B plane verification | 0x00=Disabled (default) 0x01=Enabled
0x13 | Japan M/S/U code treatment | 0x00 = M/S/U wildcard enabled (default) 0x01 = M/S/U wildcard disabled
0x14 to 0x16 | Reserved |
0x17 | SCCP User Part Availability | 0x00 = Unavailability 0x01 = Available locally (default) 0x02 = Available remotely 0x03 = Invalid
0x18 | TUP User Part Availability | 0x00 = Unavailable 0x01 = Available locally (default) 0x02 = Available remotely 0x03 = Invalid
0x19 | ISUP User Part Availability | 0x00 = Unavailable 0x01 = Available locally (default) 0x02 = Available remotely 0x03 = Invalid
0x1A | User Part 0x06 Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x1B | User Part 0x07 Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available Remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x1C | MTP Test User Part Availability | 0x00 = Unavailable 0x01 = Available locally (default) 0x02 = Available remotely 0x03 = Invalid
0x1D | User Part 0x09 Availability | 0x00 = Unavailable (default for ITU variant) 0x01 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x1E | User Part 0x0A Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x1F | User Part 0x0B Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x20 | User Part 0x0C Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x21 | User Part 0x0D Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x22 | User Part 0x0E Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x23 | User Part 0x0F Availability | 0x00 = Unavailable (default for ITU variant) 0x02 = Available remotely 0x03 = Invalid (default for ANSI and Japan variant)
0x24 to 0x26 | Reserved |
0x27 | SCCP User Part Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x28 | TUP User Part Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x29 | ISUP User Part Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2A | User Part 0x06 Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2B | User Part 0x07 Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2C | MTP Test User Part Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2D | User Part 0x09 Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2E | User Part 0x0A Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x2F | User Part 0x0B Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x30 | User Part 0x0C Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x31 | User Part 0x0D Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x32 | User Part 0x0E Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x33 | User Part 0x0F Multihost Routing | 0x00 = force routing to port 0x3142 0x01 = force routing to port 0x3143 0x02 = force routing to port 0x3144 0x03 = force routing to port 0x3145 0x04 = force routing to port 0x3146 0xFF = force routing disabled (default)
0x34 | Anonymous TFC Treatment | 0x00 = Disabled 0x01 = Enabled (default)
0x35 | Ericsson TFC Treatment | 0x00 = Disabled (default) 0x01 = Enabled
0x36 | SCCP Message OPC Validation | 0x00 = Do not transmit to user part (default) 0x01 = Transmit to user part (SCCP)

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)
A grouping of nodes in a network (as defined by point code), usually grouped by geographical region.
See Signaling System Number Seven.
Message Transfer Part level 3 - network level
See Programmable Protocol Language.
Telephone User Part
See Integrated Services Digital Network User Part.
See Message Transfer Part.