TCAP TUSI PPL Event Indications and Requests (ITU)

All the ANSI and ITU TCAP TC-primitives are PPL events to/from the PPL component TCAP TUSI.

Event ID | Event
--- | ---
0x01 | TC-BEGIN
0x02 | TC-CONTINUE
0x03 | TC-END
0x04 | TC-UNI
0x05 | TC-U-ABORT
0x06 | TC-P-ABORT (Indication only)
0x0C | TC-RESULT-L
0x0D | TC-RESULT-NL
0x0E | TC-U-ERROR
0x0F | TC-L-CANCEL (Indication only)
0x12 | TC-U-REJECT
0x13 | TC-L-REJECT (Indication only)
0x14 | TC-R-REJECT (Indication only)
0x15 | TC-INVOKE
0x16 | TC-U-CANCEL (Request only)
0x17 | TC-NOTICE (Indication only)
0x18 | BAD REJECT RECEIVED (Indication only)
0x1E | TCAP-RESTART
0x1F | TCAP-MESSAGE NOT COMPLETE (Indication only)
0x20 | TCAP-DIALOG TIMEOUT (Indication only)
0x21 | TCAP INITIATED ABORT
0x31 | TC-UNI-PRIMITIVE-SET
0x32 | TC-BEGIN-PRIMITIVE-SET
0x33 | TC-CONTINUE-PRIMITIVE-SET
0x34 | TC-END-PRIMITIVE-SET

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)
See Transaction Capability Application Part.
See Programmable Protocol Language.