0x275A Generic Command
(Interworking Only)

Use this TLV to send a generic command to the network entity to perform some predefined command codes.

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x275A
2, 3 | Length Variable
4, 5 | Value[0,1] Generic Command Length MSB, LSB
6, 7 | Value[2,3] Generic Command MSB, LSB
: | :
: | Value[n] Generic Command MSB, LSB

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Most Significant Bit
Least Significant Bit