You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Download Begin BRecord 0x009B

Download Begin BRecord 0x009B

Configuration API Messages

SwitchKit Name

DownloadBeginBRecord

Type

EXS API and SwitchKit API message

Description

Download Begin BRecord 0x009B

This message should not be sent by the host to standby CSP 2000 Matrix Cards, since the CSP Matrix Series 3 CardCSP Matrix Series 3 Cards receive their loads from the TFTP download.

However, you can use this message to configure active CSP 2000 Matrix Cards.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

} XL_DownloadBeginBRecord;

C++ Class

class XLC_DownloadBeginBRecord : public XLC_OutboundMessage {

public:

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x009B) | 3, 4 | Message Type (0x009B)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 | Checksum | 8, 9 | Status MSB, LSB
10 | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
Least Significant Bit