0x12 Signaling Route Test Control DPC

Used in:
0x1E and 0x001E Generic PPL ICBs in PPL Event Request message

Byte | Description
0 | Tag 0x12 Signaling Route Test Control DPC
1 | Length 0x01
2 | Value[0] 0x02

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Destination Point Code