0x09D2 Global Title Entry Query Response

Used in:
SS7 SCCP/TCAP Query message

Byte | Description
0, 1 | Tag 0x09D2 Global Title Entry Query Response
2, 3 | Length Variable Note: If you attempt to query either a Global Title Entry that does not exist, the TLV length in the response will be one byte consisting of null data.
4 | Value[0] State 0 = Idle 1 = In service 2 = Pending_Add 3 = Pending_Del
5 | Value[1] Translation Result Option
6 | Value[2] Translation Result 1 See Table Translation Result Format
7 | Value[3] Translation Result 2 (If it exists.) See Table Translation Result Format .

See Signaling System Number Seven.
See Transaction Capability Application Part.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.