0x293C NPDI SIP Authorization Password

Use this TLV to specify the password used to generate the Authorization header for an outgoing request when the CSP receives a 401 response.

Used in:
0x0033 NPDI Universal ICB in:
Route Control message

Byte | Description
0, 1 | Tag 0x293C
2, 3 | Length Variable
4-n | Value[0-n] NULL Terminated ASCII string for password

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
American Standard Code for Information Interchange