You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Record File Stop 0x0120

Record File Stop 0x0120

SwitchKit Name

RecordFileStop

Type

EXS API and SwitchKit API message

Description

Record File Stop 0x0120

NOTE: This message applies to the DSP Series 2 card only.

Use this message to end a current record file session.

Sent by

Host Application

Related API Messages

Record File Start, Record File Modify

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[253];

} XL_RecordFileStop;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE reserved6[13];

UBYTE AddrInfo[251];

} XL_RecordFileStopAck;

C++ Class

class XLC_RecordFileStop : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

XBYTE getConferenceID() const;

void setConferenceID(XBYTE x);

XBYTE getParentConferenceID() const;

void setParentConferenceID(XBYTE x);

XBYTE getChildConferenceID() const;

void setChildConferenceID(XBYTE x);

XBYTE getSpan() const;

void setSpan(XBYTE x);

UBYTE getChannel() const;

void setChannel(UBYTE x)

};

C++ Class Response

class XLC_RecordFileStopAck : public XLC_OutboundMessage {

public:

unsigned short getStatus() const

void setStatus(unsigned short x)

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

XBYTE getConferenceID() const;

void setConferenceID(XBYTE x);

XBYTE getParentConferenceID() const;

void setParentConferenceID(XBYTE x);

XBYTE getChildConferenceID() const;

void setChildConferenceID(XBYTE x);

XBYTE getSpan() const ;

void setSpan(XBYTE x) ;

UBYTE getChannel() const;

void setChannel(UBYTE x);

;

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x00NN)
3, 4 | Message Type (0x0120) | 3, 4 | Message Type (0x0120)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB) 0x0001 Invalid TLV Data Software can't find the TLV Data Buffer. This can also occur if the Data for a TLV is out of range. 0x0003 Invalid number of TLVs There are no TLVs in the message. 0x0004 Invalid TLV Length The TLV length is different from what is expected. 0x0006 Invalid TLV Unknown TLV 0x000D Mandatory TLVs missing One or more mandatory TLVs are missing Also see Common Response Status Values.
Number of AEs to follow | : | AIB Same as message
AEs Use one of the following: 0x0D Channel 0x55 Conference ID 0x45 Child Conference ID and (if recording a conference) 0x01 Slot | : | Checksum
| Checksum

Digital Signal Processor
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.