You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Default CPA Tone Pattern Parameters

Default CPA Tone Pattern Parameters

Ringback

Ringback
Pattern ID | 0x01
Tone Group ID | 0x00
Configuration Bits | 0x00
CPA Result on Pattern Loss | 0x80
Interval Cycles to Match | 1
Interval Cycles to Report | 3
Interval Descriptor Count | 2
Interval Descriptors |
Tone Interval 0: Tone ID | 0x02
Reserved | 0x00
Minimum Filter (ms) | 600
Maximum Filter (ms) | 2200
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 2800
Maximum Filter (ms) | 5000

Double Ringback

Double Ringback |
--- | ---
Pattern ID | 0x02
Tone Group ID | 0x00
Configuration Bits | 0x00
CPA Result on Pattern Loss | 0x80
Interval Cycles to Match | 1
Interval Cycles to Report | 3
Interval Descriptor Count | 4
Tone Interval 0: Tone ID | 0x02
Reserved | 0x00
Minimum Filter (ms) | 420
Maximum Filter (ms) | 580
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 400
Tone Interval 2: Tone ID | 0x02
Reserved | 0x00
Minimum Filter (ms) | 420
Maximum Filter (ms) | 580
Tone Interval 3: Tone ID | 0x00
Reserved | 0
Minimum Filter (ms) | 2000
Maximum Filter (ms) | 2500

Busy

Busy |
--- | ---
Pattern ID | 0x03
Tone Group ID | 0x00
Configuration Bits | 0x00
CPA Result on Pattern Loss | 0x03
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 2
Tone Interval 0: Tone ID | 0x05
Reserved | 0x00
Minimum Filter (ms) | 420
Maximum Filter (ms) | 580
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 420
Maximum Filter (ms) | 580
Tone Interval 2: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |
Tone Interval 3: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |

Reorder

Reorder |
--- | ---
Pattern ID | 0x04
Tone Group ID | 0x00
Configuration Bits | 0x00
CPA Result on Pattern Loss | 0x04
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 2
Tone Interval 0: Tone ID | 0x05
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 300
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 300
Tone Interval 2: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |
Tone Interval 3: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |

PBX intercept

PBX Intercept |
--- | ---
Pattern ID | 0x05
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x05
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 2
Tone Interval 0: Tone ID | 0x03
Reserved | 0x00
Minimum Filter (ms) | 100
Maximum Filter (ms) | 300
Tone Interval 1: Tone ID | 0x06
Reserved | 0x00
Minimum Filter (ms) | 100
Maximum Filter (ms) | 300
Tone Interval 2: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |
Tone Interval 3: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |

SIT Intercept

SIT Intercept |
--- | ---
Pattern ID | 0x06
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x06
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x07
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 350
Tone Interval 1: Tone ID | 0x09
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 350
Tone Interval 2: Tone ID | 0x0B
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 3: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |

Vacant Code

Vacant Code |
--- | ---
Pattern ID | 0x07
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x07
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x08
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 1: Tone ID | 0x09
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 350
Tone Interval 2: Tone ID | 0x0B
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 3: Tone ID |
Reserved |
Minimum Filter (ms) |
Maximum Filter (ms) |

Reorder LEC

Reorder LEC |
--- | ---
Pattern ID | 0x08
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x08
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x07
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 350
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 2: Tone ID | 0x0B
Reserved | 0
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460

No Circuit LED

No Circuit LED |
--- | ---
Pattern ID | 0x09
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x09
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x08
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 1: Tone ID | 0x0A
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 2: Tone ID | 0x0B
Reserved | 0
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460

Reorder Carrier

Reorder Carrier |
--- | ---
Pattern ID | 0x0A
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x0A
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x08
Reserved | 0x00
Minimum Filter (ms) | 200
Maximum Filter (ms) | 350
Tone Interval 1: Tone ID | 0x09
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 2: Tone ID | 0x0B
Reserved | 0
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460

No Circuit Carrier

No Circuit Carrier |
--- | ---
Pattern ID | 0x0B
Tone Group ID | 0x00
Configuration Bits | 0x02
CPA Result on Pattern Loss | 0x0B
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 3
Tone Interval 0: Tone ID | 0x07
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 1: Tone ID | 0x09
Reserved | 0x00
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460
Tone Interval 2: Tone ID | 0x0B
Reserved | 0
Minimum Filter (ms) | 300
Maximum Filter (ms) | 460

PBX Dialtone

PBX Dialtone |
--- | ---
Pattern ID | 0x0C
Tone Group ID | 0x00
Configuration Bits | 0x01
CPA Result on Pattern Loss | 0x0C
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 7
Tone Interval 0: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 2: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 3: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 4: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 5: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 80
Maximum Filter (ms) | 120
Tone Interval 6: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 500
Maximum Filter (ms) | 0

Standard Dial Tone

Standard Dial Tone |
--- | ---
Pattern ID | 0x0D
Tone Group ID | 0x00
Configuration Bits | 0x05
CPA Result on Pattern Loss | 0x0D
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 1
Tone Interval 0: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 500
Maximum Filter (ms) | 0

CPC Detection

CPC Detection |
--- | ---
Pattern ID | 0x0E
Tone Group ID | 0x00
Configuration Bits | 0x01
CPA Result on Pattern Loss | 0x0E
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 1
Tone Interval 0: Tone ID | 0x01
Reserved | 0x00
Minimum Filter (ms) | 1500
Maximum Filter (ms) | 0

Fax

Fax |
--- | ---
Pattern ID | 0x13
Tone Group ID | 0x00
Configuration Bits | 0x00
CPA Result on Pattern Loss | 0x13
Interval Cycles to Match | 1
Interval Cycles to Report | 1
Interval Descriptor Count | 2
Tone Interval 0: Tone ID | 0x11
Reserved | 0x00
Minimum Filter (ms) | 425
Maximum Filter (ms) | 575
Tone Interval 1: Tone ID | 0x00
Reserved | 0x00
Minimum Filter (ms) | 2550
Maximum Filter (ms) | 3450

See Private Branch Exchange.