You are here: PPL Developer’s Guide > 6 SS7 Atomic Functions > SCCP SCRC (0x0066)

SCCP SCRC (0x0066)

The following atomic functions are used by the PPL component, SCRC (SCCP Routing Control - 0x0066).

Atomic Functions

.

AF Number | 92
Name | Test whether Global Title Translation (GTT) is allowed for local sub-system.
Description | Tests whether GTT is needed and the sub-system number (SSN) is allowed to do GTT locally.
Arg1 | <Not Used>
Arg2 | <Not Used>
Results | PPLevINT_EVENT_1 if yes. PPLevINT_EVENT_0 if GTT is not needed

AF Number | 93
Name | SCRC Global Title Translation
Description | This function performs GTT, returns the success or failure status, and determines whether to perform further treatment to the address after the GTT.
Arg1 | <Not Used>
Arg2 | <Not Used>
Results | PPLevINT_EVENT_0: success PPLevINT_EVENT_1: No translation for an address of such nature PPLevINT_EVENT_2: No translation for this specific address PPLevINT_EVENT_3: SSN failure PPLevINT_EVENT_4: SCCP unequipped PPLevINT_EVENT_5: MTP failure PPLevINT_EVENT_6: MSG overlength with new CDPA PPLevINT_EVENT_7: Support UMTS calling party address treatment. PPLevINT_EVENT_7: After GTT operation needed

AF Number | 94
Name | Universal mobile telecommunications systems (UMTS) calling party address (CGPA) treatment
Description | Supports UMTS CGPA treatment.
Arg1 | <Not Used>
Arg2 | <Not Used>
Result | PPLevINT_EVENT_0 if success PPLevINT_EVENT_6 if fail

AF Number | 95
Name | SCRC updates the called party address (CDPA).
Description | Updates CDPA in the internal chained buffer with new CDPA results from GTT.
Arg1 | <Not Used>
Arg2 | <Not Used>
Result | Void

See Programmable Protocol Language.
See Atomic Function.
See Message Transfer Part.