0x37 Query Multi-Host Status

Used in:
Multi-Host Configure message

ICB Type | 0x01 (Action)
ICB ID | 0x37
Data Length | Variable
Data[0–3] | Default Host ID (4 bytes)
Data[4] | Status 0x00 - Disabled 0x01 - Enabled

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Information Control Block.