0x0071 Virtual VoIP Channel

Indicates to the router that a virtual VoIP channel will be hunted.
Used in:
PPL Table Download message
0x1E and 0x001E Generic PPL ICBs in Route Control message

Byte | Description
0, 1 | Tag 0x0071
2, 3 | Length 0x0002
4,5 | Value[0-1] 0x0000

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.