0x05FE Resource Point Statistics

This TLV may be returned in the response to the Statistics Query message. Note: TLV 0x05F9, query type 0404 is only valid while addressing the CSP Matrix Series 3 Card s lot to query Resource Points. It does not work, if you address the DSP Series 2 card slot to query Resource Points.

Byte | Description
0, 1 | Tag: 0x05FE Resource Point Statistics
2, 3 | Length: 0x0010
4-7 | Value[0-3]:Points Configured
8-11 | Value[4-7]: Points Available
12-15 | Value[8-11]: Minimum Points Available
16-19 | Value[12-15]: Average Points Available

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor