L3P Control Protocol PPL Timers (0x008F)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Waiting for Port Control Acknowledge | 1 seconds
0x02 | Waiting for Common Control Acknowledge | 1 seconds
0x03 | Waiting for Datalink Connection Establish | 4 seconds

See Programmable Protocol Language.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."