You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Matrix Status Report 0x00E5

Matrix Status Report 0x00E5

SwitchKit Name

DeviceServerStatusReport

Type

EXS API and SwitchKit API message

Description

Matrix Status Report 0x00E5

This is an unsolicited message sent from the CSP Matrix Series 3 Card to the Host in different situations. This is generally caused by an IP Signaling Series 3 card interaction about which the Host requires information.

NOTE: This message supports a feature of a Dialogic product other than SwitchKit. For this reason, the message is not to be used in a SwitchKit only environment.

Sent by

CSP

SwitchKit Code

C Structure

typedef struct {

unsigned short DeviceServer;

UBYTE TLVCount;

UBYTE Data[222];

} XL_DeviceServerStatusReport;

C++ Class

class XLC_DeviceServerStatusReport : public XLC_InboundMessage {

public:

unsigned short getDeviceServer() const;

void setDeviceServer(unsigned short x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x00E5) | 3, 4 | Message Type (0x00E5)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
Number of AEs to follow
AE 0x73 IP Signaling Series 3 Card ID
: | Number of TLVs to follow | 10 | Checksum
: | TLV 0x0003 Protocol Type 0x000B V5 Cpath Assignment 0x0080 IP Signaling Series 3 Card Status
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.