L3P BCC Configuration Bytes

Byte | Description | Values (* Default)
--- | --- | ---
0x01 | Send Deallocate Request to L3 upon receiving Channel Remove message from PSTN | * 0x00 = Send Deallocate Request to L3 0x01 = Do not send Deallocate Request
0x02 | Number of Allocation Request resends before giving up (send Channel Request reject to PSTN) | *0x00 =Default number of resends
0x03 | Reserved |
0x04 | Reserved |
0x05 | Override the BCC Channels that are allocated and this can be set only from LE Side. | * 0x00 = Do not override 0x01 = Over

Public Switched Telephone Network